



Part 1: Create FTP traffic.



Step 1: Activate the sniffing device.




Step 2: Remotely connect to the FTP server.












Part 2: Investigate the FTP Traffic




Part 3: View syslog Messages

Step 1: Remotely connect to Router2.



From PC-B



From PC-C

